TECHNICAL DATA

**Cordless circular saw SCM 22-A case** #2024449

Battery voltage22 V

Rated voltage21.6 V

No-load speed3500 tours/minute

Battery type Li-ion

Triaxial vibration value for sawing into metal (ah,M) 1.2 m/s² 1

A-weighted emission sound power level 88 dB (A) 2

Blade diameter - range160 - 165 mm

Weight according to EPTA Procedure 01/2003 4 kg

Max. cutting depth 57 mm

Arbor size 20 mm

Base material Metal and metal sandwich

Variable speed switch Yes

Electric brake Yes